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ARCHITECTURAL SPECIFICATION
SL-10 Manual Closing Pedestrian Gate – Chrome Finish 

SECTION 11 14 00 – Pedestrian Control Equipment (Gates/Turnstiles)

PART I – GENERAL

1.01 SECTION INCLUDES
A. This section covers the furnishing and installation of a SL-10 gate with a 36” opening. 
B. For further information, call the factory at +1 909.423.4143 and ask for the technical support department; or email support@alvaradomfg.com.

1.02 RELATED SECTIONS
A. Section 084000 – Entrances and Storefronts
B. Section 087100 – Door Hardware
C. Section 083456 – Security Gates

1.03 QUALITY ASSURANCE
A. Manufacturer shall be a company specializing in the supply of pedestrian gates with a minimum of 10 years’ experience.
B. Installer shall have a minimum of one year experience installing similar equipment, or shall supply a factory representative during installation of the product.

1.04 SUBMITTALS
A. Submit manufacturer’s descriptive literature for specified equipment, including options.
B. Provide dimensional layout, installation instructions, electrical and communication connections and anchoring instructions.
C. Provide shop drawings, if required.

1.05 DELIVERY, STORAGE AND HANDLING
A. Deliver materials to job site in manufacturer’s packaging undamaged, complete with installation instructions.
B. Store off ground, under cover, protected from weather, construction activities and debris.
C. Use forklift and pallet jack equipment as required for moving. 

1.06 PROJECT/SITE CONDITIONS
Install the SL-10 on a level concrete pad.

1.07 WARRANTY
Alvarado warranties its products against defects in material and workmanship for a period of one (1) year from the date of invoicing. The warranty covers defects in materials and workmanship and does not cover freight, labor or incidental costs. Obtain full warranty terms from Alvarado. 

PART II – PRODUCTS

2.01 MANUFACTURER
Alvarado Mfg. Co., Inc. 12660 Colony Street, Chino, CA 91710.

2.02 PRODUCT
SL-10 Manual Closing Pedestrian Gate, no substitutions. Features of the gate shall include: single direction passage; manual-closing design; 36” passage width; chrome plated finish.

2.03 FACTORY TESTING 
A. Product shall be fully tested at the factory prior to shipment. 
B. Check all mechanical connections.
C. Inspect product finish. Touch up prior to shipment.

2.04 CONSTRUCTION
A. Gate Arm: 16-gauge steel tubes, chrome plated finish.
B. Hinge Post: 11-gauge steel, chrome plated finish.

PART III – EXECUTION

3.01 SITE EXAMINATION
A. Inspection: Installer must examine the installation location and advise the Contractor of any site conditions inconsistent with proper installation of the product. These conditions include but are not limited to the following:
1. Gate must be installed on a level concrete pad.
Installation shall not begin until unacceptable conditions are rectified.
B. Installation: Install gates in accordance with manufacturer’s instructions. 
C. Adjustment: Installer shall adjust gates for proper performance after installation.
D. Instruction: A factory trained installer shall demonstrate to the owner’s maintenance crew the proper operation and the necessary service requirements of the equipment, including exterior maintenance. 
E. Cleaning: Clean gate and area carefully after installation to remove excess caulk, dirt and labels. 


Note: Alvarado Mfg. Co., Inc. reserves the right to change this specification at any time without notice.
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