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ARCHITECTURAL SPECIFICATION
Quick Queue Wall Mount Stanchions

[NOTE TO SPECIFIER, SELECT PRODUCT MODEL DEPENDING ON DESIRED FINISH]

AVAILABLE FINISHES
07-5330 – Black Matte Finish
07-5350 – Mirror Finish

SECTION 11 14 00 – Pedestrian Control Equipment 

PART I – GENERAL

1.01 SECTION INCLUDES
A. This section covers the furnishing and installation of Quick Queue wall mount stanchions. 
B. For further information, contact Alvarado at +1 909.591.8431 or email information@alvaradomfg.com.
 
1.02 QUALITY ASSURANCE
A. Manufacturer shall be a company specializing in the supply of asset protection products with a minimum of 10 years of experience.

1.03 SUBMITTALS
A. Submit manufacturer’s descriptive literature for specified equipment, including options.
B. Provide dimensional layout and installation instructions.
C. Provide shop drawings, if required.

1.04 DELIVERY, STORAGE AND HANDLING
A. Deliver materials to job site in manufacturer’s packaging undamaged, complete with installation instructions.
B. Store off-ground, under cover, protected from weather, construction activities and debris.
C. Use forklift, pallet jack or equivalent equipment for moving. 

1.05 PROJECT/SITE CONDITIONS
[bookmark: _GoBack]Install the Quick Queue wall mount stanchions on level surfaces only.

1.06 WARRANTY
Alvarado Manufacturing Co., Inc. warrants the Quick Queue wall mount stanchions from defects in material or workmanship, for a period of ONE YEAR from date of shipment. Complete details of the warranty are available from Alvarado by request. 

PART II – PRODUCTS

2.01 MANUFACTURER
Alvarado Mfg. Co., Inc. 12660 Colony Street, Chino, CA 91710.

2.02 PRODUCT
Quick Queue wall mount stanchions, no substitutions.

2.03 CONSTRUCTION
A. Housing: The housing is a 2.5” OD tube fabricated from 20-gauge cold-rolled steel (black matte finish) or 22-gauge stainless steel (mirror finish). The housing is 4.75” in height and includes a 4.125” x 4.5” mounting plate. Mounting hardware is included.
B. Belt: Belts are 2” wide and available in lengths of 7’ and 13’. Standard belt colors are black, red, yellow, burgundy, blue and green for 7’ belts and black, red and yellow for 13’ belts. 

2.04 EQUIPMENT
A. General: Quick Queue wall mount stanchions are wall-mounted barriers designed to provide crowd and patron control.

2.05 FINISHES

[NOTE TO SPECIFIER: SELECT the finish desired]

A. Black matte finish
B. Mirror finish

2.06 OPTIONS

[NOTE TO SPECIFIER: Select the options desired]

A. Belt Colors: Custom colors are available for volume orders.
B. Belt Imprints: Belts can be ordered with silkscreened messages.

2.07 FACTORY TESTING 
A. Product shall be fully tested at the factory to ensure proper functionality.
B. Inspect product finish. Touch up prior to shipment.

PART III – EXECUTION

3.01 SITE EXAMINATION
A. Inspection: Installer must examine the installation location and advise the contractor of any site conditions inconsistent with proper installation of the product. Installation shall not begin until unacceptable conditions are rectified. These conditions include but are not limited to the following:
1. Product must be installed on level surfaces.
B. Installation: The installer should perform the installation, in consultation with the owner or end user, following the practices and installation guidelines that come with the product. 
C. Cleaning: Clean metal surfaces carefully after installation to remove dirt and labels.

Note: This specification includes recommended options. Alvarado Mfg. Co., Inc. reserves the right to change this specification at any time without notice. 
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